LAND SURVEY REFERENCE REPORT
State Archives and Library Division
FOR OFFICIAL USE ONLY:





Kansas State Historical SocietyRevised 4/9/2025

6425 SW Sixth Avenue, Topeka, KS, 66615-1099
Phone: (785) 272-8681, ext. 254          Fax: (785) 272-8682


Land Surveyor:   ________________________
Company:               ________________________
Street Address:  ________________________
City & State:         ________________________
ZIP Code:                 ________________________

License Number:     ________________________
Project Number:     ________________________
Phone Number:       ________________________
Date of Survey:        ________________________
County of Survey:  ________________________
This report is filed as a (check only one):
[bookmark: _Hlk131777707]   ☐	Survey Reference Report (K.S.A. 58-2011a) 	    ☐	Notice of Endangerment Activity (K.S.A. 58-2011b)
  	There is a $4.00/corner filing fee for Survey Reference Reports and Notices of Endangerment Activity (K.A.R. 188-4-4a).
   ☐	Notice of Completion of Endangerment Activity & Report of Restoration (K.S.A. 58-2011c)
This may only be filed after filing a prior Notice of Endangerment Activity.  There is no filing fee.
Original Notice of Endangerment Activity was filed on ____________.

LOCATION CODE OF MARKER IN TOWNSHIP (see illustration below for help):  ____
Legal Description: ________________________		Section: ____		Township: ____South	Range: ____
Survey Datum (if known): ________________________	North: ____________		East: ____________
Corner Status Prior to Survey:	☐ Existent		☐ Obliterated		☐ Lost		☐ Endangered
Monument Condition:		☐ Found		☐ Set			☐ Reset	☐ Found Record
Detailed Monument Description: __________________________________________________________________
REFERENCE MARKS AND MEASUREMENTS (no symbols or abbreviations):
NOTE: ALL MEASUREMENTS ARE      ☐  HORIZONTAL      ☐  SLOPED      UNLESS NOTED OTHERWISE.
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DETAILED METHOD OF RECOVERY OR ESTABLISHMENT: 


IDENTIFYING A MARKER

To identify the location of a marker in a township, use the following standard alpha-numeric grid to designate an identifier for a given section corner or intersection.

For Example: The southwest corner of Section 26 would be designated by the identifier 17V. This is the LOCATION CODE OF MARKER IN TOWNSHIP.
The original signature and date shall be across the Land Surveyor’s Professional seal.
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Surveyor’s Signature & Date

